//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

.Set READY_VAR = 01
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 01
 Receive	Data:84 A9 61 00 02 00 10 00
pause 4000
Command ID:	VOCODER_CMODE
Send	Command: 84 A9 61 00 02 00 02 0A
Receive	Data:84 A9 61 00 02 00 02 00

Command ID:	NXDN_SR
Send	Command: 84 A9 61 00 02 06 77 01
Receive Data:   84 A9 61 00 02 06 77 00 
Command ID:	NXDN_CALL_OPTION
Send	Command: 84 A9 61 00 06 06 47 82 00 00 00 00
Receive Data:   84 A9 61 00 02 06 47 00
Pause 1000
Command ID:	WORK_MODE_DUPLEX
Send	Command: 84 A9 61 00 04 00 18 03 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 02
Receive	Data:84 A9 61 00 02 00 1A 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 01
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	NXDN_DATA_FRAME
Send command: 84 a9 61 00 11 00 77 01 43 a0 00 0b 40 01 00 20 00 01 00 01 00 00 00 00 
Receive Data: 84 a9 61 00 01 20 43
Command ID:   NXDN_DATA_FRAME
Send command: 84 a9 61 00 0e 00 43 c0 00 0a 56 01 00 20 00 01 00 01 00 00
Receive Data: 84 a9 61 00 01 20 43
//Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 24 30 77 01 43 00 00 1E 40 10 00 00 00 00 00 00 00 00 01 00 20 00 01 00 01 00 00 00 01 00 20 00 01 00 01 00 00 00
Receive	Data:84 A9 61 00 24 30 77 01 43 00 00 1E 56 01 00 20 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
PAUSE 2000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 80 F6 80 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 81 F6 80 01
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 82 F6 80 02
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 83 F6 80 03
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 84 F6 80 04
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 85 F6 80 05
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 86 F6 80 06
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 87 F6 80 07
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 88 F6 80 08
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 89 F6 80 09
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8A F6 80 0A
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8B F6 80 0B
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8c F6 80 0C
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8d F6 80 0D
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8e F6 80 0E
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 8f F6 80 0F
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 E8
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 05 F6 00 9a
//Receive	Data:84 A9 61 00 06 30 08 03 05 F6 00 9c
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 0a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 0a F6 01 3a
//Receive	Data:84 A9 61 00 06 30 08 03 0a F6 01 38
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 0a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 10 F6 01 f4
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 30 F6 05 dc
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 40 F6 07 d0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 50 F6 09 c4
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 60 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 60 F6 0b b8
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 03 70 F3
//Receive	Data:84 A9 61 00 02 00 08 00
//Receive	Data:84 A9 61 00 06 30 08 03 70 F6 0d ac
//pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 00 70 F3
//Receive	Data:84 A9 61 00 02 00 08 00
//Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00

//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 03 7a F3
//Receive	Data:84 A9 61 00 02 00 08 00
//Receive	Data:84 A9 61 00 06 30 08 03 7a F6 0e e4
//pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 00 7a F3
//Receive	Data:84 A9 61 00 02 00 08 00
//Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00


Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 E8
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 E8
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00

pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 EE
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 EE
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 F2
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 F2
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 F6
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 F6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 F9
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 21 F6 03 F9
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 04 01
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 21 F6 04 01
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 04 05
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 21 F6 04 05
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 04 09
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 21 F6 04 09
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 04 0B
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 21 F6 04 09
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 03 E8
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 20 F6 03 E8
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 00 80
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 04 F6 00 7f
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 00 70
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 04 F6 00 6f
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 00 6c
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 03 F6 00 6b
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00
pause 1000


Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 07 20 F3 00 68
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 03 F6 00 64
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 06 30 08 03 FF A6 00 00


//Command ID:	VOCODER_CMODE
//Send	Command: 84 A9 61 00 02 00 02 08
//Receive	Data:84 A9 61 00 02 00 02 00

pause 4000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 7a F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7a F3
Receive	Data:84 A9 61 00 02 00 08 00

pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 06 00 08 05 20 F3 03 E8
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 06 00 08 05 20 F3 00 68
//Receive	Data:84 A9 61 00 02 00 08 00
//pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 00 20 F3
//Receive	Data:84 A9 61 00 02 00 08 00

//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 06 00 08 05 20 F3 00 80
//Receive	Data:84 A9 61 00 02 00 08 00
//pause 1000
//Command ID:	VOCODER_TONE
//Send	Command: 84 A9 61 00 04 00 08 00 20 F3
//Receive	Data:84 A9 61 00 02 00 08 00

Command ID: NXDN_DATA_FRAME
Send command: 84 a9 61 00 11 00 77 c1 43 a0 00 0b 40 08 00 20 00 01 00 01 00 00 00 00
Receive       Data:84 a9 61 00 01 20 43
Pause 100
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 24 30 77 01 43 00 00 1E 40 10 00 00 00 00 00 00 00 00 08 00 20 00 01 00 01 00 00 00 08 00 20 00 01 00 01 00 00 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00


