//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
//3917+wolfson+1847SETTING
.Set READY_VAR = 01
.Set CODEC_VAR = 02
.Set OPTION_VAR1 = 71
.Set OPTION_VAR2 = 00
.Set MODEL_VAR = 51

//2928+TICODEC+3700SETTING
//.Set READY_VAR = 02
//.Set CODEC_VAR = 02
//.Set OPTION_VAR1 = 71
//.Set OPTION_VAR2 = 80
//.Set MODEL_VAR = 31

Command ID:	Q_SW_VER
Send	Command: 84 A9 61 00 01 23 32 00
Receive	    Data:84 A9 61 00 0C 23 32 0A 56 32 2E 30 31 2E 30 30 50 36